Odes UTVs Factory Warranty Details of Coverage

|  |  |  |
| --- | --- | --- |
| **Covered Parts** | Description | Duration |
| **800cc Motor** | Engine | 24 Months |
| **Transmission** | Transmission | 12 Months |
| **Electrical** | EFI, Fuel, Electrical Components | 12 Months |
| **Suspension** | Shocks | 12 Months |
| **Brake** | Caliper | 12 Months |
| **Exhaust** | Headers, Pipe, Muffler | 12 Months |
| **Frame** | Frame | 12 Months |
| **Clutch** | CVT/Manual Clutch | 12 Months |

Vehicle Owner’s Responsibilities:

* Vehicle Owner’s must properly use, maintain and care for their UTV as defined in the Owners Manual.
* Owner must service their UTV as defined in the Owners Manual.
* Owner must maintain all service records of work performed to their UTV.
* Only an authorized ODES UTV dealer or service center can perform warranty repairs.
* Periodic service and inspections are considered regular maintenance and not reimbursable.
* All warranty repairs require authorization by ODES UTV.
* All ODES UTV products require a dealer pre-delivery inspection and assembly to ensure proper operation, safety, and warranty validation.
* Owners must break-in their vehicle before high performance use or the vehicle can be subject to warranty non-approval. The break in period is half throttle or 4000 rpm for the first 3 hours of initial use or no more than 25mph on the 800cc motor.
* Warranty starts from date of purchase by the consumer from their OEDS UTV dealer.
* Vehicle must be registered by the ODES UTV dealer the UTV was purchased through within 5 days of purchase.

General Parts Not Covered

Battery, Spark Plugs, Cables, Drive Belts, Air Filters, Front / Rear Brake Pads, Bushings, Light Bulbs, Fuses, Rubber Parts, Seats, Misc. Hardware, Mirrors, Rubber Gaskets, Hubs, Front / Rear Tires, Front / Rear Rims, Gear & Engine Oil, Front / Rear Brake Rotors, Brake / Clutch Levers, Steering Stem Bearings, Steering universals,Buggy Floor/ Plastics / Fuel Filters / Steering Wheel and Motor Mount Bushings, any other part that is considered wear and tear.